IVC bt878 Series - Readme Instructions
Version 1.7.1.2504 - June 4, 2004

I. SYSTEM REQUIREMENTS

Software:
Windows 98 Second Edition, Windows Millennium, Windows 2000 or Windows XP

Hardware:
IBM or IBM-compatible PC with at least one empty PCI slot, IVC bt878 Series Card


II. INSTALLATION INSTRUCTIONS

To install the software for your IVC Card, you could choose one of the following two methods.

Method A:

1. Run ieisetup.exe within this package.
2. Turn your system off.
3. Insert your IVC Card to empty PCI slots.
4. Restart your system.

Method B:

1. Turn your system off.
2. Insert your IVC Card to empty PCI slots.
3. Restart your system.
3. Click "Cancel" for all pop-up "New Device Found" dialogs.
4. Run ieisetup.exe within this package to install the software for your IVC Card.

Note:

1. In either case, setup program will install DirectX 8.1 automatically if there is no or older DirectX installed in your system.
2. If you want to install the driver manually without using ieisetup.exe, please make sure to install DirectX 8.1 if there is no or older DirectX installed in your system.
3. If you want to reinstall or upgrade the driver, please do remember to uninstall the old one first.


III. UNINSTALLATION INSTRUCTIONS

To remove this software, please follow below steps:

1. Open the Control Panel by clicking Settings from Start Menu.
2. Open the "Add/Remove Program" and select "IVC bt878 Series" from the list.
3. Click on the "Add/Remove" button and follow the instructions to complete uninstallation.
